***Tech Tip***



***POWERED by PROPANE***

***From your friends at New York Bus Sales***

**Complaint - The High Idle does not disengage when the emergency brake is released.**

**Cause - This is “by design” – The High Idle will only disengage when the service brake is applied.**

**Correction - None Needed**

**PLEASE NOTE – There may be a question of what happens if the unit is put into gear without first depressing the service brake and the High Idle is engaged – This DOES NOT create an issue as the service brake MUST be applied or the transmission “Range Inhibit” takes over and will not shift the unit into gear!**

***Contact Our Service Department with Any Questions***

***CHITTENANGO*** *– phone 800-962-5768 or*

*Daryl Wallace :* [*dwallace@newyorkbussales.com*](mailto:dwallace@newyorkbussales.com)

*Brian Lamaitis :* [*blamaitis@newyorkbussales.com*](mailto:blamaitis@newyorkbussales.com)

***ROCHESTER*** *– phone 800-463-3232 or*

*Gary Chichester:* [*gchichester@newyorkbussales.com*](mailto:gchichester@newyorkbussales.com)

***ALBANY*** *– phone 866-867-1100 or*

*Ben Reiling:* [*breiling@newyorkbussales.com*](mailto:breiling@newyorkbussales.com)

Steve Searles: [ssearles@newyorkbussales.com](mailto:ssearles@newyorkbussales.com)

***WARRANTY*** *– 800-962-5768 ext.237*

*Morgan Jenkins:* [*mjenkins@newyorkbussales.com*](mailto:mjenkins@newyorkbussales.com)

THANK YOU TO CHRIS FROM SHARON SPRINGS CENTRAL SCHOOL FOR POINTING THIS OUT

TO US!

****

**ALL of our Tech Tips can be found on the New York Bus Sales website at**

[**http://www.newyorkbussales.com/pages/bulletins.cfm**](http://www.newyorkbussales.com/pages/bulletins.cfm)